{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["汇总"],"not_rendered":{"charts":0,"images":28,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"汇总","index":0,"n_rows":467,"n_cols":8,"rows_kept":467,"cut":false,"hidden":false,"merged":[[110,2,111,2],[232,0,233,0],[232,1,233,1],[265,0,266,0],[265,1,266,1],[247,0,249,0],[247,1,249,1],[243,1,246,1],[210,1,215,1],[210,0,215,0],[351,6,360,6],[324,0,329,0],[324,1,329,1],[467,0,467,2],[424,0,425,0],[424,1,425,1],[351,1,360,1],[351,0,360,0],[334,0,340,0],[373,0,374,0],[12,1,13,1],[42,0,45,0],[42,1,45,1],[125,0,128,0],[125,1,128,1],[97,0,98,0],[97,1,98,1],[29,0,32,0],[29,1,32,1],[61,0,63,0],[138,0,139,0],[138,1,139,1],[131,0,132,0],[131,1,132,1],[64,0,66,0],[64,1,66,1],[2,0,11,0],[2,1,11,1],[12,0,13,0],[61,1,63,1],[48,0,50,0],[48,1,50,1],[38,0,39,0],[51,0,52,0],[51,1,52,1],[57,0,59,0],[76,0,78,0],[38,1,39,1],[40,0,41,0],[40,1,41,1],[25,0,26,0],[25,1,26,1],[53,0,56,0],[57,1,59,1],[79,1,80,1],[23,0,24,0],[23,1,24,1],[82,0,84,0],[182,1,197,1],[182,0,197,0],[123,1,124,1],[82,1,84,1],[67,0,69,0],[67,1,69,1],[133,1,136,1],[208,1,209,1],[143,0,144,0],[99,0,101,0],[99,1,101,1],[102,0,104,0],[102,1,104,1],[106,0,109,0],[106,1,109,1],[123,0,124,0],[145,1,146,1],[147,0,148,0],[147,1,148,1],[112,2,113,2],[114,2,115,2],[117,0,118,0],[117,1,118,1],[119,0,120,0],[119,1,120,1],[133,0,136,0],[260,0,261,0],[260,1,261,1],[267,0,271,0],[155,0,156,0],[155,1,156,1],[216,1,221,1],[216,0,221,0],[198,0,202,0],[198,1,202,1],[206,0,207,0],[305,7,306,7],[305,0,306,0],[305,1,306,1],[267,1,271,1],[272,0,275,0],[272,1,275,1],[298,1,299,1],[256,2,258,2],[253,0,254,0],[253,1,254,1],[222,0,223,0],[222,1,223,1],[236,0,242,0],[236,1,242,1],[256,0,258,0],[256,1,258,1],[243,0,246,0],[302,0,303,0],[319,0,321,0],[319,1,321,1],[365,0,366,0],[365,1,366,1],[330,1,333,1],[330,0,333,0],[14,0,16,0],[14,1,16,1],[87,0,88,0],[87,1,88,1],[91,1,95,1],[91,0,95,0],[76,1,78,1],[73,1,75,1],[73,0,75,0],[79,0,80,0],[143,1,144,1],[145,0,146,0],[0,1,0,7],[27,0,28,0],[27,1,28,1],[70,1,72,1],[70,0,72,0],[18,1,19,1],[18,0,19,0],[53,1,56,1],[110,0,115,0],[110,1,115,1],[129,0,130,0],[129,1,130,1],[121,1,122,1],[121,0,122,0],[208,0,209,0],[163,1,178,1],[163,0,178,0],[206,1,207,1],[149,0,150,0],[149,1,150,1],[180,0,181,0],[180,1,181,1],[457,0,458,0],[375,0,376,0],[426,0,427,0],[426,1,427,1],[375,1,376,1],[225,0,227,0],[225,1,227,1],[373,1,374,1],[276,0,279,0],[276,1,279,1],[280,0,281,0],[280,1,281,1],[286,0,287,0],[286,1,287,1],[298,0,299,0],[459,0,460,0],[459,1,460,1],[368,0,369,0],[368,1,369,1],[439,0,440,0],[341,1,349,1],[341,0,349,0],[334,1,340,1],[361,1,364,1],[361,0,364,0],[229,1,231,1],[229,0,231,0],[313,1,318,1],[313,0,318,0],[302,1,303,1],[449,1,450,1],[449,0,450,0],[378,0,380,0],[378,1,380,1],[406,0,407,0],[406,1,407,1]],"flags":["formulas_cached_only"]}
["附件1","上海市强制检定计量器具检定收费标准"]
["专业序号","计量器具名称","准确度或等级","测量范围","计费\n单位","收费标准(元)","检定周期","备注"]
["C-001-001","量块","二等","≤100mm","块",165,"1年"]
[null,null,"三等","0.5 ～ 100mm","块",40,"1年"]
[null,null,"三等","> 100 ～ 500mm","块",85,"1年"]
[null,null,"三等","> 500 ～ 1000mm","块",130,"1年"]
[null,null,"四等","0.5 ～ 100mm","块",29.75,"1年"]
[null,null,"四等","> 100 ～ 500mm","块",70,"1年"]
[null,null,"四等","> 500 ～ 1000mm","块",105,"1年"]
[null,null,"五等","0.5 ～ 100mm","块",15,"1年"]
[null,null,"五等","> 100 ～ 500mm","块",59.5,"1年"]
[null,null,"五等","> 500 ～ 1000mm","块",90,"1年"]
["C-002-002","标准玻璃线纹尺","一等","0 ～ 200mm","支",900,"1年"]
[null,null,"二等","0 ～ 200mm","支",500,"1年"]
["C-003-003","标准金属线纹尺","一等","0 ～ 1000mm","支",1350,"1年"]
[null,null,"二等","0 ～ 1000mm","支",750,"1年"]
[null,null,"三等","0 ～ 1000mm","支",425,"1年"]
["C-004-004","标准钢卷尺","5μm+5L","≤5m","支",210,"1年"]
["C-005-005","钢卷尺（含带锤钢卷尺）","I级","0 ～ 200m","支/5m",25,"1年","5m以上每米加2元   "]
[null,null,"II级","0 ～ 200m","支/5m",15,"1年","5m以上每米加1元   "]
["C-006-006","铁路轨距尺","±0.10mm","1428 ～ 1470mm","支",70,"1年"]
["C-007-007","套管尺","±（0.4+0.3L）mm","600 ～ 4500mm","米",85,"1年"]
["C-008-008","多齿分度台",null,"0°～ 360°","台",600,"1年"]
["C-009-009","正多面棱体","3等","0 ～ 360°","面",35,"1年"]
[null,null,"4等","0 ～ 360°","面",25,"1年"]
["C-010-010","测角仪","1″～ 2″","0°～ 360°","台",1250,"1年"]
[null,null,"> 2″～ 5″","0°～ 360°","台",525,"1年"]
["C-011-011","角度块","0级，1级","0°～ 360°","角",35,"1年"]
[null,null,"2级","0°～ 360°","角",29.75,"1年"]
["C-012-012","平面平晶","二等","D:150mm","块",350,"1年"]
[null,null,"一级，二级","100mm＜D≤150mm","块",100,"1年"]
[null,null,"一级，二级","60mm＜D≤100mm","块",75,"1年"]
[null,null,"一级，二级","≤60mm","块",50,"1年"]
["C-013-013","平面等厚干涉仪","0.02μm","0 ～ 200mm","台",265,"1年"]
["C-014-014","研磨面平尺","≤ 0.4μm","≤ 300mm","支",300,"1年"]
["C-015-015","水平仪检定器",0.05,"2mm/m","台",240,"1年"]
["C-016-016","直角尺检定仪","±0.002mm","0 ～ 400mm","台",435,"1年"]
["C-017-017","百分表检定仪","±0.004mm","0 ～ 25mm","台",210,"1年"]
["C-018-018","千分表检定仪","±2μm","0 ～ 2mm","台",350,"1年"]
[null,null,null,"0 ～ 5mm","台",565,"1年"]
["C-019-019","电子水平仪","电容：≤（1+A/50）μm\n电感：≤1分度","≥ 0.005mm/m","台",195,"1年"]
[null,null,"电容：≤（1+A/50）μm\n电感：≤1分度","< 0.005mm/m","台",290,"1年"]
["C-020-020","标准环规","二等","≥ 3 ～ 50mm","只",85,"1年"]
[null,null,"二等","> 50 ～ 80mm","只",135,"1年"]
[null,null,"三等","≥ 3 ～ 50mm","只",70,"1年"]
[null,null,"三等","> 50 ～ 80mm","只",75,"1年"]
["C-021-021","经纬仪检定装置","±2\"","0 ～ 360°","台",4200,"1年"]
["C-022-022","水准仪检定装置",null,null,"台",4200,"1年"]
["D-001-023","直流数字电压表","0.001 ～ 0.002级","0 ～ 1000V","台",525,"1年"]
[null,null,"0.005级","0 ～ 1000V","台",420,"1年"]
[null,null,"0.01 ～ 0.05级","0 ～ 1000V","台",315,"1年"]
["D-002-024","直流标准电压源","0.001 ～ 0.005级","0 ～ 1000V","台",700,"1年"]
[null,null,"0.01级及以下","0.1 ～ 1000V","台",520,"1年"]
["D-003-025","直流电流电压标准源","0.001级","0.1 ～ 1000V，0 ～ 1A","每功能",680,"1年"]
[null,null,"0.002 ～ 0.005级","0.1 ～ 1000V，0 ～ 1A","每功能",510,"1年"]
[null,null,"0.01 ～ 0.05级","0.1 ～ 1000V，0 ～ 1A","每功能",340,"1年"]
[null,null,"0.1级及以下","0.1 ～ 1000V，0 ～ 1A","每功能",300,"1年"]
["D-004-026","电压电流电阻校准仪","0.001级、0.002 ～ 0.005级","0 ～ 1000V，0 ～ 10A","每功能",515,"1年","只检定直流部分 "]
[null,null,"0.01 ～ 0.05级","0 ～ 1000V，0 ～ 10A","每功能",340,"1年","只检定直流部分 "]
[null,null,"0.1级及以下","0 ～ 1000V，0 ～ 10A","每功能",255,"1年","只检定直流部分 "]
["D-005-027","数字电流表","0.01级以下","0.1mA ～ 2A","台 ",280,"1年"]
["D-006-028","直流电流表（指针式）","0.1级","0 ～ 50A","基本\n量限",175,"1年","交直流两用检定加收基本量限50%，每加一个量限加收75元"]
[null,null,"0.2级","0 ～ 50A","基本\n量限",125,"1年","交直流两用检定加收基本量限50%，每加一个量限加收60元"]
[null,null,"0.5级","0 ～ 50A","基本\n量限",75,"1年","交直流两用检定加收基本量限50%，每加一个量限加收40元"]
["D-007-029","交流电流表（指针式）","0.1级","0 ～ 20A","基本\n量限",175,"1年","每加一个量限加收75元"]
[null,null,"0.2级","0 ～ 20A","基本\n量限",125,"1年","每加一个量限加收60元"]
[null,null,"0.5级","0 ～ 20A","基本\n量限",100,"1年","每加一个量限加收40元"]
["D-008-030","直流电压表（指针式）","0.1级","0 ～ 1000V","基本\n量限",175,"1年","交直流两用检定加收基本量限50%，每加一个量限加收75元"]
[null,null,"0.2级","0 ～ 1000V","基本\n量限",125,"1年","交直流两用检定加收基本量限50%，每加一个量限加收60元"]
[null,null,"0.5级","0 ～ 1000V","基本\n量限",75,"1年","交直流两用检定加收基本量限50%，每加一个量限加收40元"]
["D-009-031","交流电压表（指针式）","0.1级","0 ～ 1000V","基本\n量限",175,"1年","每加一个量限加收75元"]
[null,null,"0.2级","0 ～ 1000V","基本\n量限",125,"1年","每加一个量限加收60元"]
[null,null,"0.5级","0 ～ 1000V","基本\n量限",100,"1年","每加一个量限加收40元"]
["D-010-032","直流功率表","0.1级","0 ～ 1000V，0 ～ 10A","基本\n量限",200,"1年","交直流两用检定加收基本量限50%，每加一个量限加收75元"]
[null,null,"0.2级","0 ～ 1000V，0 ～ 10A","基本\n量限",150,"1年","交直流两用检定加收基本量限50%，每加一个量限加收60元"]
[null,null,"0.5级","0 ～ 1000V，0 ～ 10A","基本\n量限",125,"1年","交直流两用检定加收基本量限50%，每加一个量限加收40元"]
["D-011-033","交流功率表（指针式）","0.1级","0 ～ 1000V，0 ～ 20A","基本\n量限",200,"1年","每加一个量限加收75元"]
[null,null,"0.2级","0 ～ 1000V，0 ～ 20A","基本\n量限",150,"1年","每加一个量限加收60元"]
[null,null,"0.5级","0 ～ 1000V，0 ～ 20A","基本\n量限",100,"1年","每加一个量限加收40元"]
["D-012-034","标准电池组","一等","（1.0186000 ～ 1.0186700）V","只",280,"1年"]
[null,null,"二等","（1.0186000 ～ 1.0186700）V","只",200,"1年"]
["D-013-035","标准电池","0.005 ～ 0.01级","（1.01855 ～ 1.01868）V","只",175,"1年"]
["D-014-036","标准电阻","一等","10-3  ～ 105Ω","只",315,"1年"]
[null,null,"二等","10-3  ～ 105Ω","只",200,"1年"]
[null,null,"0.01级及以下","10-3 ～ 105Ω","只",130,"1年"]
["D-015-037","大功率标准电阻","0.01级及以下","10-3 ～ 10-1Ω","只",175,"1年"]
["D-016-038","直流数字电阻表","0.002级及以下","10Ω ～ 10MΩ","台",360,"1年"]
["D-017-039","标准电容器","0.01 ～ 0.02级","1 ～ 106pF","只",280,"1年"]
[null,null,"0.05级","1 ～ 106pF\n0.01pF ～ 1μF","只",200,"1年"]
["D-018-040","标准电感器","0.05级","1μH ～ 1H","只",100,"1年"]
["D-019-041","直流比较仪式电位差计","0.0001级","0 ～ 2.111111V","台",875,"1年"]
["D-020-042","直流电位差计","0.0005级","0.01μV ～ 2.1111110V","台",1200,"1年"]
[null,null,"0.001 ～ 0.002级","0 ～ 2.111111V","台",700,"1年"]
[null,null,"0.005级","0 ～ 2.111111V","台",350,"1年"]
[null,null,"0.01 ～ 0.02级","0 ～ 2.111111V","台",250,"1年"]
[null,null,"0.05级及以下","（0.000001 ～ 1.0550）V","台",250,"1年"]
["D-021-043","直流比较仪式电桥","0.0001级","10-5 ～ 106Ω","台",875,"1年"]
["D-022-044","直流电桥","0.01 ～ 0.02级","10-5 ～ 106Ω","台",350,"1年","直流双桥加收50%"]
[null,null,"0.1级及以下","10-3 ～ 105Ω","台",300,"1年","直流双桥加收50% "]
["D-023-045","直流测温电桥","0.01级","（0.0010 ～ 555.5600）Ω","台",1045,"1年"]
[null,null,"0.02级","（0.0010 ～ 555.5600）Ω","台",810,"1年"]
[null,null,"0.05级","（0.0010 ～ 555.5600）Ω","台",520,"1年"]
["D-024-046","直流电阻箱","0.001 ～ 0.005级","10-2 ～ 105Ω","点",25,"1年"]
[null,null,"0.01 ～ 0.05级","10-3 ～ 105Ω","点",8.5,"1年"]
[null,null,"0.1级及以下","10-3 ～ 105Ω","点",4,"1年"]
["D-025-047","直流分压箱","0.01 ～ 0.02级","电压上限≤1.5kV","台",280,"1年","基本点为10点，超过10点，每点加收50元"]
["D-026-048","电压互感器","0.005级","0 ～ 35kV","基本\n量限",240,"2年","每加一个量限，加收100元，超35kV的检定加收200元"]
[null,null,"0.01 ～ 0.02级","0 ～ 35kV","基本\n量限",200,"2年","每加一个量限，加收75元，超35kV的检定加收150元"]
[null,null,"0.01 ～ 0.05级","10V ～ 35kV","基本\n量限",200,"2年","每加一个量限，加收75元"]
[null,null,"0.05级","0 ～ 35kV","基本\n量限",150,"2年","每加一个量限，加收50元，超35kV的检定加收100元"]
["D-027-049","电流互感器","0.001 ～ 0.005级","2kA以下","基本\n量限",200,"2年","每加一个量限，加收60元"]
[null,null,null,"2 ～ 10kA","基本\n量限",325,"2年","每加一个量限，加收150元"]
[null,null,"0.01 ～ 0.05级","2kA以下","基本\n量限",175,"2年","每加一个量限，加收60元"]
[null,null,null,"2 ～ 10kA","基本\n量限",235,"2年","每加一个量限，加收90元"]
[null,null,"0.1 ～ 0.5级","2kA以下","基本\n量限",100,"2年","每加一个量限，加收40元"]
[null,null,null,"2 ～ 10kA","基本\n量限",190,"2年","每加一个量限，加收60元"]
["D-028-050","互感器校验仪","1.0级，2.0级","150V，100V，100/   V，5A，1A","台",385,"1年"]
["D-029-051","标准单相电能表","0.05级","220V，100V，1～5A","基本价/台",250,"1年","每点加收50元"]
[null,null,"0.1 ～ 0.2级","220V，100V，1～5A","基本价/台",175,"1年","每点加收35元"]
["D-030-052","三相标准电能表","0.02级，0.05级","电压：3×380V\n电流：3×5A","基本价/台",250,"1年","每点加收50元"]
[null,null,"0.1 ～ 0.2级","电压：3×380V\n电流：3×5A","基本价/台",175,"1年","每点加收35元"]
["D-031-053","单相电能表","1级及以下","电压：220V\n电流：100A及以下","台",50,"10年"]
[null,null,"1级及以下","电压：220V\n电流：100A及以下","台",120,"10年","现场检定  "]
["D-032-054","感应式三相电能表","1级及以下","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",100,"4年"]
[null,null,"1级及以下","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",245,"4年","现场检定  "]
["D-033-055","电子式三相电能表","0.5级，0.2级","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",200,"5年"]
[null,null,"1级及以下","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",120,"5年"]
[null,null,"0.5级，0.2级","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",250,"5年","现场检定   "]
[null,null,"1级及以下","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",245,"5年","现场检定   "]
["D-034-056","单相多费率电能表","1级及以下","电压：220V\n电流：100A及以下","台",75,"10年"]
[null,null,"1级及以下","电压：220V\n电流：100A及以下","台",155,"10年","现场检定 "]
["D-035-057","三相多费率电能表","1级及以下","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",170,"4年"]
[null,null,"1级及以下","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",300,"4年","现场检定"]
["D-036-058","电子式三相多功能电能表","0.5级，0.2级","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",410,"5年"]
[null,null,"1级及以下","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",345,"5年"]
[null,null,"0.5级，0.2级","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",360,"5年","现场检定  "]
[null,null,"1级及以下","电压：3×（57 ～ 380）V\n电流：3×120A及以下","台",350,"5年","现场检定  "]
["D-037-059","单相电能表检定装置","0.05级","电压：48 ～ 600V\n电流：0.1 ～ 100A","台",1955,"1年"]
["D-038-060","三相电能表检定装置","0.05 ～ 0.1级","100V，220V，380V，0～50A","台",2450,"1年"]
[null,null,"0.2 ～ 0.3级","100V，220V，380V，0～50A","台",1925,"1年"]
["D-039-061","接地电阻测量仪","1.0 ～ 3.0级","0.01～1000Ω","台",250,"2年","测量电流5A以下"]
["D-040-062","绝缘电阻表（兆欧表）","5% ～ 10%","2GΩ以下","台",80,"2年"]
["G-001-063","光强度标准灯","1.8%，二级","1000W以下","支",350,"1年"]
["G-002-064","总光通量标准白炽灯","2%，二级","1000W以下","支",420,"1年"]
[null,null,"2.8%，三级","1000W以下","支",250,"1年"]
["G-003-065","总光通量标准荧光灯","≤3%，一级","1000W以下","支",315,"1年"]
[null,null,"≤3.8%，二级","1000W以下","支",280,"1年"]
["G-004-066","总光通量标准荧光高压汞灯","≤4%，一级","1000W以下","支",425,"1年"]
[null,null,"≤4.8%，二级","1000W以下","支",335,"1年"]
["G-005-067","亮度计","5%，一级","0.1 ～ 3000cd/m2","点",270,"1年"]
[null,null,"10%，二级","0.1 ～ 3000cd/m2","点",250,"1年"]
["G-006-068","遮光筒式亮度计",0.1,"0.02 ～ 1000cd/m2","点",270,"1年"]
["G-007-069","激光小功率计","2%（k=2）","0.1 ～ 100mW","档",240,"1年"]
["G-008-070","激光中功率计","2%（k=2）","0.1 ～ 150W","档",280,"1年"]
["G-009-071","医用激光源","5%（k=2）","0.1mW ～ 150W","台",280,"1年"]
["G-010-072","照度计","一级 ","0.1 ～ 3000lx","档",250,"1年"]
[null,null,"二级  ","2 ～ 3000lx","档",225,"1年"]
["G-011-073","紫外辐射照度计","±20%","（2×10-5 ～ 2×10-2）W/cm2","台",520,"1年"]
["G-012-074","焦度计","0.02D，0.06D","（-25 ～ +25）D","台",315,"1年"]
["G-013-075","验光镜片箱","0.04D","（-20 ～ +20）D","片",3,"2年"]
["G-014-076","验光机","Δ＝±（0.25～0.50）D","（-20 ～ +20）D","台",350,"1年"]
["G-015-077","镜向光泽度计（仪）","1光泽单位","0 ～ 150光泽单位","角度档",225,"1年"]
["G-016-078","镜向光泽度板","0.8光泽单位","0 ～ 150光泽单位","角度档",225,"1年"]
["L-001-079","砝码","E2级","0.05 ～ 500mg","只",125,"2年"]
[null,null,"E2级","1 ～ 500g","只",175,"2年"]
[null,null,"E2级","1 ～ 20kg","只",250,"2年"]
[null,null,"F1级","1 ～ 500mg","只",75,"1年"]
[null,null,"F1级","1 ～ 500g","只",100,"1年"]
[null,null,"F1级","1 ～ 20kg","只",150,"2年"]
[null,null,"F2级","1 ～ 500mg","只",50,"1年"]
[null,null,"F2级","1 ～ 500g","只",75,"1年"]
[null,null,"F2级","1 ～ 20kg","只",125,"2年"]
[null,null,"F2级","50 ～ 100kg","只",875,"2年"]
[null,null,"M1级","1 ～ 500mg","只",30,"1年"]
[null,null,"M1级","1 ～ 500g","只",40,"1年"]
[null,null,"M1级","1 ～ 20kg","只",60,"1年"]
[null,null,"M1级","50 ～ 100kg","只",250,"1年"]
[null,null,"M11级","0.5t","只",210,"1年"]
[null,null,"M11级","1t","只",255,"1年"]
["L-002-080","谷物水份测定仪","一级及以下","5 ～ 50%","台",100,"1年"]
["L-003-081","戥秤",null,"≤ 250g","台",10,"1年"]
[null,null,null,"> 250g","台",10,"1年"]
["L-004-082","机械天平","1 ～ 3级","2 ～ 20g","台",150,"1年"]
[null,null,"1 ～ 3级","100 ～ 200g","台",225,"1年"]
[null,null,"1 ～ 3级","1 ～ 5kg","台",250,"1年"]
[null,null,"1 ～ 3级","10 ～ 50kg","台",260,"1年"]
[null,null,"4 ～ 6级","100 ～ 200g","台",150,"1年"]
[null,null,"4 ～ 6级","1 ～ 5kg ","台",175,"1年"]
[null,null,"4 ～ 6级","10～50kg","台",200,"1年"]
[null,null,"4 ～ 6级","500kg ","台",350,"1年"]
[null,null,"4 ～ 6级","1000 ～ 2000kg","台",700,"1年"]
[null,null,"4 ～ 6级","3000 ～ 5000kg","台",1750,"1年"]
[null,null,"7 ～ 10级","100 ～ 200g","台",125,"1年"]
[null,null,"7 ～ 10级","1 ～ 5kg","台",125,"1年"]
[null,null,"7 ～ 10级","10 ～ 50kg","台",150,"1年"]
[null,null,"7 ～ 10级","1000kg以下","台",315,"1年"]
[null,null,"7 ～ 10级","1000 ～ 2000kg","台",525,"1年"]
[null,null,"7 ～ 10级","3000 ～ 5000kg","台",1225,"1年"]
["L-005-083","电子天平","I","2 ～ 500g\n1 ～ 20kg","台",420,"1年"]
[null,null,"II","100 ～ 500g\n1 ～ 20kg","台",350,"1年"]
[null,null,"II","100 ～ 200kg ","台",805,"1年"]
[null,null,"II","> 1000kg ","台",1225,"1年"]
[null,null,"III","100 ～ 500g\n1 ～ 20kg","台",250,"1年"]
["L-006-084","扭力天平","II","1kg以下","台",75,"1年"]
["L-007-085","架盘天平","III","100g ～ 10kg","台",30,"1年"]
["L-008-086","比重天平","II","100g以下","台",25,"1年"]
["L-009-087","非自动衡器（商贸用秤）",null,"≤ 30kg","台",20,"1年"]
[null,null,null,"> 30kg ～ 500kg","台",40,"1年"]
["L-010-088","价格标签秤（条形码打印电子计价秤）","III、IV","≤ 30kg","台",40,"1年"]
[null,null,"III、IV","> 30kg","台",60,"1年"]
["L-011-089","非自动衡器（电子台、吊秤）","III","≤ 60kg","台",160,"1年"]
[null,null,"III","> 60 ～ 1000kg","台",280,"1年"]
[null,null,"III","> 1000 ～ 3000kg","台",700,"1年"]
[null,null,"IV","≤ 60kg","台",100,"1年"]
[null,null,"IV","> 60 ～ 1000kg","台",200,"1年"]
[null,null,"IV","> 1000 ～ 3000kg","台",350,"1年"]
["L-012-090","非自动衡器（机械台、吊秤）","III","≤ 60kg","台",160,"1年"]
[null,null,"III","> 60 ～ 1000kg","台",280,"1年"]
[null,null,"III","> 1000 ～ 3000kg","台",700,"1年"]
[null,null,"IV","≤ 60kg","台",100,"1年"]
[null,null,"IV","> 60 ～ 1000kg","台",200,"1年"]
[null,null,"IV","> 1000 ～ 3000kg","台",350,"1年"]
["L-013-091","非自动衡器（邮用秤）","III、IV","≤ 30kg","台",50,"1年"]
[null,null,"III、IV","> 30kg","台",60,"1年"]
["L-014-092","电子汽车秤","III、IV","20 ～ 150t","台",1400,"1年","20t以上每t加收25元"]
["L-015-093","地上衡（地中衡）","III、IV","5t以下","台",700,"1年"]
[null,null,"III、IV","> 5 ～ 10t","台",1400,"1年"]
[null,null,"III、IV","> 10 ～ 20t","台",2000,"1年","20t以上每t加收25元"]
["L-016-094","非连续累计自动秤","0.2，0.5","< 100t/h","台",1750,"1年"]
["L-017-095","电子皮带秤","0.5，1.0，2.0","≤ 1000t/h","台",1400,"1年"]
[null,null,"0.5，1.0，2.0","1000 ～ 6000t/h","台",2100,"1年"]
[null,null,"0.5，1.0，2.0","> 6000t/h","台",2800,"1年"]
["L-018-096","定量包装秤","0.1，0.2，0.5","≤ 25kg","台",1400,"1年"]
[null,null,"0.1，0.2，0.5","> 25kg","台",2100,"1年"]
["L-019-097","定量包装商品净含量",null,"质量、体积、长度标注","件",20]
["L-020-098","标准洛氏、表面洛氏、布氏、维氏、显微、肖氏硬度块","标准","HRC、HRA、HRB，\nHBS（W） 25-650，\nHV5、HV10、HV30、HV100、\nHV0.05～HV1，\n（30±4）HSD、（60±4）HSD、（95±4）HSD","块",100,"1年"]
["L-021-099","标准金属量器","2.5×10-4","1 ～ 10L","台",280,"3年"]
[null,null,"2.5×10-4","20L","台",525,"3年"]
[null,null,"2.5×10-4","50L","台",840,"3年"]
[null,null,"2.5×10-4","100L","台",1050,"3年"]
[null,null,"2.5×10-4","200L ～ 500L","台",1350,"3年"]
[null,null,"2.5×10-4","1000L","台",1575,"3年"]
[null,null,"2.5×10-4","2000L","台",2800,"3年"]
["L-022-100","工作金属量器","（1 ～ 0.5）×10-3","1 ～ 20L","台",300,"2年"]
[null,null,"（1 ～ 0.5）×10-3","50 ～ 500L","台",700,"2年"]
[null,null,"（1 ～ 0.5）×10-3","1000L","台",1000,"2年"]
[null,null,"（1 ～ 0.5）×10-3","2000L","台",1400,"2年"]
["L-023-101","标准玻璃量器","二等","< 100mL","只",150,"3年"]
[null,null,"二等","100 ～ 250mL","只",200,"3年"]
[null,null,"二等","500 ～ 10000mL","只",280,"3年"]
["L-024-102","立式计量罐","0.1% ～ 0.2%","10 ～ 100000m3","座",700,"4年","基价基础上，每1m3加收1元"]
["L-025-103","卧式计量罐",0.004,"10 ～ 200m3","座",500,"4年","基价基础上，每1m3加收1元"]
["L-026-104","球形计量罐",0.003,"10 ～ 1000m3","座",875,"4年","基价基础上，每1m3加收1元"]
["L-027-105","船舶计量舱","0.3% ～ 0.5%","载重量 < 5000t","舱",1225,"10年","基价基础上，每1m3加收6元"]
[null,null,"0.3% ～ 0.5%","载重量 > 5000t","舱",1225,"10年","基价基础上，每1m3加收5元"]
["L-028-106","汽车计量罐车",0.0025,"1 ～ 10m3","辆",630,"4年","基价基础上，每1m3加收50元"]
["L-029-107","定量灌装机",null,"单头","台",470,"1年"]
[null,null,null,"30 ～ 50头","台",875,"1年"]
[null,null,null,"50 ～ 120头","台",1225,"1年"]
["L-030-108","转速表检定装置",null,null,"台",750,"1年"]
["L-031-109","出租汽车计价器检定装置 ","0.1级","0.1 ～ 9999.9","台",420,"1年","本机"]
[null,null,"0.5级","0 ～ 9999","台",630,"1年","使用误差"]
["L-032-110","出租汽车计价器","-4% ～ +1%","（20 ～ 100000）r/min","台",45,"1年"]
["L-033-111","雷达测速仪","1km/h","10 ～ 250km/h","台",150,"1年"]
["L-034-112","转矩转速测量装置","0.1级，0.2级，0.5级，1.0级","1 ～ 5000N·m","台",700,"1年"]
["L-035-113","负荷传感器","0.1级","2MN以下","台",440,"1年"]
[null,null,"0.5级","2MN以下","台",325,"1年"]
["L-036-114","标准测力仪","3×10-3，0.3级","100 ～ 6000N","台",300,"1年"]
[null,null,"3×10-3，0.3级","30 ～ 300kN","台",400,"1年"]
[null,null,"3×10-3，0.3级","100 ～ 1000kN","台",455,"1年"]
[null,null,"3×10-3，0.3级","200 ～ 2000kN","台",525,"1年"]
[null,null,"3×10-3，0.3级","300 ～ 3000kN","台",875,"1年"]
["L-037-115","密度计","一等","（0.65 ～ 200）g/cm3","点",40,"1年"]
[null,null,"二等","（0.65 ～ 200）g/cm3","点",30,"1年"]
[null,null,"工作用","（0.65 ～ 200）g/cm3","点",20,"1年"]
[null,null,"实验室用","（0.65 ～ 200）g/cm3","点",40,"1年"]
["L-038-116","酒精计","一等","0 ～ 100%","点",40,"1年"]
[null,null,"二等","0 ～ 100%","点",30,"1年"]
[null,null,"实验室用","0 ～ 100%","点",35,"1年"]
[null,null,"工作用","0 ～ 100%","点",20,"1年"]
["L-039-117","海水密度计","一等","（1.00 ～ 1.04）相对密度","点",40,"1年"]
[null,null,"工作用","（1.00 ～ 1.04）相对密度","点",20,"1年"]
["L-040-118","压电加速度计",null,null,"台",455,"1年"]
["L-041-119","标准压电加速度计",null,null,"台",750,"1年"]
["L-042-120","振动测量仪",null,null,"台",350,"1年"]
["L-043-121","振动冲击测量仪",null,null,"台",350,"1年"]
["L-044-122","活塞式压力计","一等","< 250MPa","台",600,"2年"]
[null,null,"二等，三等","< 250MPa","台",420,"2年"]
["L-045-123","单双活塞式压力真空计","一等，二等","（-0.1 ～ 0.25）MPa","台",500,"2年"]
["L-046-124","数字血压计检定仪","0.1级及以下","0 ～ 40kPa","只",460,"1年"]
["L-047-125","弹性式血压计标准器","0.16级及以下","0 ～ 40kPa","台",245,"1年"]
["L-048-126","标准血压计","0.16级","0 ～ 40kPa","台",245,"1年"]
["L-049-127","血压计（表）","±0.5kPa","0 ～ 40kPa","台",10,"半年"]
["L-050-128","数字式电子血压计（静态）","±0.5kPa","0 ～ 40kPa","台",35,"1年"]
["L-051-129","压陷式眼压计","±（0.3 ～ 1.0）格","0 ～ 1mm，0 ～ 20格","台",40,"1年"]
["L-052-130","液体压力计","一、二、三等","0 ～ 10kPa，25kPa","台",240,"1年"]
["L-053-131","补偿式微压计","二等","0 ～ 1500Pa，0 ～ 2500Pa","台",280,"2年"]
["L-054-132","倾斜式微压计","工作用","2000Pa ","台",240,"1年"]
["L-055-133","精密压力表","0.25级，0.4级，0.6级","＜5MPa","块",100,"1年"]
[null,null,"0.25级，0.4级，0.6级","＞5MPa","块",125,"1年"]
["L-056-134","精密真空表","0.25级，0.4级，0.6级","（-0.1 ～ 0）MPa","只",150,"1年"]
["L-057-135","弹簧管式精密压力表和真空表","0.25级及以下","上限100 ～ 250MPa","只",300,"1年"]
["L-058-136","一般压力表","1级及以下","（-0.1 ～ 60）MPa","只",40,"半年"]
[null,null,"1级及以下","上限 100 ～ 250MPa","只",100,"半年"]
["L-059-137","浮标式氧气吸入器","2.5级、4级","压力：0 ～ 25MPa \n流量：（1 ～ 10）L/min","台",60,"半年"]
["L-060-138","气体流量计","≥0.5%","DN：≤100mm","台",3500,"1年","天然气介质 4.0MPa"]
[null,null,"≥0.5%","DN：150 ～ 250mm","台",14000,"1年"]
["L-061-139","涡轮流量计",null,"DN：15 ～ 100mm","台",700,"1年","以空气为检定介质"]
["L-062-140","转子流量计","1.5 ～ 4级","DN：6 ～ 150mm","台",200,"1年"]
["L-063-141","速度式流量计","0.2% ～ 1.5%","DN：≤100mm","台",420,"1年","以原油等油品为检定介质 "]
["L-064-142","质量流量计","0.1% ～ 0.2%","DN：≤40mm","台",700,"1年","以水为检定介质"]
["L-065-143","明渠流量计","2.5% ～ 5.0%","500m3/h以上","台",800,"1年"]
["L-066-144","电磁流量计",null,"DN：15 ～ 100mm","台",1050,"1年","以空气为检定介质"]
["L-067-145","旋涡流量计","±（0.5 ～ 1.0）%","DN：25mm","台",205,"2年"]
[null,null,null,"DN：40 ～ 50mm","台",355,"2年"]
[null,null,null,"DN：80 ～ 100mm","台",705,"2年"]
[null,null,null,"DN：150 ～ 200mm","台",920,"2年"]
[null,null,null,"DN：250 ～ 300mm","台",1760,"2年"]
[null,null,null,"DN：300 ～ 400mm","台",2650,"2年"]
["L-068-146","差压式流量计","1.0级","管径：φ50mm","台",890,"1年"]
[null,null,"1.0级","管径：φ100mm","台",1785,"1年"]
[null,null,"1.0级","管径：φ1000mm","台",8715,"1年"]
["L-069-147","燃油加油机",0.003,"1 ～ 999.99L","枪",110,"半年"]
["L-070-148","LPG加气机","1级","0 ～ 60L","枪",300,"半年"]
["L-071-149","钟罩式气体流量标准装置","±（0.2 ～ 0.5）%","50L","台",1020,"3年"]
[null,null,"±（0.2 ～ 0.5）%","100L","台",1530,"3年"]
[null,null,"±（0.2 ～ 0.5）%","200L","台",1895,"3年"]
[null,null,"±（0.2 ～ 0.5）%","500L","台",3860,"3年"]
[null,null,"±（0.2 ～ 0.5）%","2000L","台",5545,"3年"]
[null,null,"±（0.2 ～ 0.5）%","5000L ～ 10000L","台",8075,"3年"]
["L-072-150","体积管","±（0.05 ～ 0.1）%","60 ～ 120L","台",2135,"3年"]
[null,null,"±（0.05 ～ 0.1）%","200 ～ 300L","台",2560,"3年"]
[null,null,"±（0.05 ～ 0.1）%","500 ～ 1100L","台",2935,"3年"]
[null,null,"±（0.05 ～ 0.1）%","> 1100 ～ 5500L","台",3385,"3年"]
["L-073-151","水流量标准装置","0.5级","DN：4 ～ 10mm","台",600,"3年"]
[null,null,"0.5级","DN：15 ～ 25mm","台",1200,"3年"]
[null,null,"0.5级","DN：40 ～ 50mm","台",2160,"3年"]
[null,null,"0.5级","DN：80 ～ 100mm","台",4920,"3年"]
[null,null,"0.5级","DN：150 ～ 200mm","台",8400,"3年"]
[null,null,"0.5级","DN：300 ～ 500mm","台",11520,"3年"]
[null,null,"0.5级","DN：1000 ～ 3000mm ","台",14160,"3年"]
["L-074-152","水表","2级","DN：15mm","台",20,"6年"]
[null,null,"3级","DN：15mm","台",15,"6年","现场检定  "]
[null,null,"2级","DN：20 ～ 25mm","台",20,"6年"]
[null,null,"2级","DN：32mm","台",25,"6年"]
[null,null,"2级","DN：40 ～ 50mm","台",60,"4年"]
[null,null,"2级","DN：80 ～ 100mm","台",65,"2年"]
[null,null,"2级","DN：150 ～ 200mm","台",100,"2年"]
[null,null,"2级","DN：250 ～ 300mm","台",175,"2年"]
[null,null,"2级","DN：400mm","台",195,"2年"]
["L-075-153","标准煤气表","±1%","1.6m3/h","只",225,"2年"]
["L-076-154","膜式煤气表","B级，±1.5%","1.6 ～ 4m3/h","只",15,"人工\n煤气\n：\n6年\n\n\n天然\n气：\n10年","在线检定  "]
[null,null,"B级，±1.5%，±6%","1.6 ～ 4m3/h","只",40]
[null,null,"A级，±2%","6m3/h","只",30,null,"在线检定  "]
[null,null,"A级，±2%,±6%","6m3/h","只",85]
[null,null,"A级，±2%","10m3/h","只",240]
[null,null,"A级，±2%","20m3/h","只",310]
[null,null,"A级，±2%","34m3/h","只",380]
[null,null,"A级，±2%","57m3/h","只",550]
[null,null,"A级，±2%","100m3/h","只",630]
[null,null,"A级，±2%","170m3/h","只",740]
["L-077-155","腰轮涡轮煤气表","±3%","300m3/h","只",1050,"2年"]
[null,null,"±3%","300m3/h以上","只",1110,"2年"]
[null,null,"≥ 1.0%","DN：25 ～ 100mm","台",1220,"2年"]
[null,null,null,"DN：150 ～ 250mm","台",1750,"2年"]
["R-001-156","标准铂电阻温度计","一等","0 ～ 419.527℃","支",700,"1年"]
[null,null,"二等","0 ～ 419.527℃","支",490,"1年"]
["R-002-157","贝克曼温度计",null,"（-20 ～ 125）℃","点",280,"1年"]
["R-003-158","标准水银温度计","一等","（-30 ～ 300）℃","点",70,"1年"]
[null,null,"二等","（-30 ～ 300）℃","点",50,"1年"]
["R-004-159","高精度实验室温度计","0.1，0.2分度","（-60 ～ 600）℃","点",50,"1年"]
["R-005-160","标准体温计","±0.03℃","35 ～ 44℃","套",420,"1年"]
["R-006-161","石油产品用温度计","±（1 ～ 2）℃","（-80 ～ 400）℃","点",50,"1年"]
["R-007-162","标准铂铑10-铂热电偶","一等","300 ～ 1300℃","支",350,"1年"]
[null,null,"二等","300 ～ 1300℃","支",315,"1年"]
["R-008-163","工作铂铑10-铂热电偶","Ⅰ级 ","0 ～ 1600℃","支",280,"1年"]
[null,null,"Ⅱ级","0 ～ 1600℃","支",250,"1年"]
["R-009-164","标准铂铑30-铂铑6热电偶","二等","1200 ～ 1600℃","支",700,"1年"]
["R-010-165","标准温度灯","标准","800 ～ 1400℃","只",400,"1年"]
[null,null,"标准","1400 ～ 2000℃","只",525,"1年"]
[null,null,"标准","2000 ～ 2500℃","只",525,"1年"]
["R-011-166","标准光学高温计","标准","800 ～ 3200℃","台",1750,"1年"]
["S-001-167","声级计","1型，2型",null,"台",280,"1年"]
["S-002-168","测试电容传声器","±3.0dB","20 ～ 20000Hz","台",415,"1年"]
["S-003-169","听力计","1 ～ 5型",null,"台",525,"1年"]
["S-004-170","声校准器","1级，2级",null,"台",200,"1年"]
["S-005-171","测试传声器","工作标准",null,"台",200,"1年"]
["S-006-172","医用超声源",null,null,"台",630,"1年"]
["W-001-173","精密交流电压校准源","±（0.02 ～ 3）%","10Hz ～ 1MHz\n1mV ～ 100V","台",1400,"1年"]
["W-002-174","脑电图机","±5%","U：1 ～ 1000μV\nf：1 ～ 60Hz","台",300,"2年"]
["W-003-175","心电图机","±5%","U：0.5 ～ 300mV\nf：0.05 ～ 60Hz","台",220,"1年"]
["W-004-176","心电监护仪","±5%","U：8μV ～ 30V\nf：0.05 ～ 200Hz","台",220,"1年"]
["W-005-177","心脑电图机检定仪","±1%","U：8μV ～ 30V\nf：0.05 ～ 200Hz","台",630,"1年"]
["W-006-178","高频Q表","±（7 ～ 15）%","Q：5 ～ 1000\nC：25 ～ 470pF","台",350,"1年"]
["W-007-179","抖晃仪",0.05,"0.001% ～ 3.999%","台",630,"1年"]
["W-008-180","同轴中功率标准","1dB","10kHz ～ 1GHz","频点",280,"1年"]
["W-009-181","通过式中功率计","1dB","10kHz ～ 1GHz","频点",280,"1年"]
["DL-001-182","医用放射性核素活度计",0.1,"37kBq ～ 3.7GBq","台",1000,"2年"]
["DL-002-183","α、β表面污染测量仪",0.25,"0.0 ～ 0.9999 ","台",400,"1年"]
["DL-003-184","X辐射防护仪器","（5 ～ 10）%","50 ～ 250kV","点",150,"1年"]
["DL-004-185","γ辐射防护仪表","（5 ～ 30）%","60Co,137Cs,226Ra,241Am\n0.3μSv/h ～ 100mSv/h","点",150,"1年"]
["DL-005-186","环境监测用X-γ辐射空气吸收剂量率仪","（10 ～ 30）%","（1×10-8 ～ 1×10-4）Gy/h","台",525,"1年"]
["DL-006-187","直读式验电型个人剂量计",0.04,"0 ～ 2×10-4C/kg","台",240,"1年"]
["DL-007-188","个人剂量与剂量率仪","10% ～ 30%","0.1μSv/h ～ 100mSv/h","台",350,"1年"]
["DL-008-189","个人场所剂量报警器","20% ～ 40%","0.1μSv/h ～ 100mSv/h","台",420,"1年"]
["DL-009-190","热释光剂量测量装置",0.05,"2μGy ～ 103Gy","台",2000,"1年"]
["DL-010-191","治疗水平电离室剂量计","2.0%，标准级","C/kg：HVL\n0.027mmAl ～ 3.0mmCu","台",2380,"1年"]
[null,null,"3.0%，工作级","C/kg：HVL\n0.027mmAl ～ 3.0mmCu","台",2030,"1年"]
["DL-011-192","60～250kV X射线治疗辐射源",0.05,"（60 ～ 250）kV X射线","台",1400,"1年"]
["DL-012-193","60Co远距离治疗辐射源",0.04,"2.58×10-7 ～ 2.58×10-1C/kg","台",1050,"1年"]
["DL-013-194","近距离γ射线后装治疗辐射源",0.04,"60Co,192Ir","台",1050,"1年"]
["DL-014-195","医用诊断X辐射源",0.1,"50 ～ 100keV","台",500,"1年"]
["DL-015-196","4～35 MeV医用加速器辐射源",0.04,"吸收剂量率：\n0.5 ～ 10Gy/min","台",2575,"1年","对单一辐射"]
["DL-016-197","医用CT扫描仪",0.1,"0.3 ～ 2.0Lp/cm","台",2050,"1年"]
["DL-017-198","X（γ）刀辐射源",0.04,"10 ～ 1000TBq","台",3040,"1年"]
["DL-018-199","放免γ计数器",0.05,"1 ～ 104Bq","台",525,"2年"]
["SP-001-200","铷原子频率标准","1×10-10","1MHz，5MHz，10MHz","台",2800,"1年"]
["SP-002-201","高稳定晶体振荡器","1×10-9","1MHz，5MHz，10MHz","台",1120,"1年"]
["SP-003-202","石英晶体振荡器","1×10-8","1MHz，5MHz，10MHz","台",980,"1年"]
["SP-004-203","机械秒表","0.01s","1s ～ 30min","只",60,"1年"]
["SP-005-204","电子秒表","1×10-6","0.01s ～ 1d","只",80,"1年"]
["SP-006-205","电子毫秒仪","1×10-7","0.1ms ～ 10s","台",450,"1年"]
["SP-007-206","时间检定仪","1×10-8","0.1ms ～ 104s","台",420,"1年"]
["SP-008-207","电子表校表仪","1×10-7","-200s/d ～ 200s/月","台",420,"1年"]
["SP-009-208","宾馆、饭店程控数字用户自动电话交换机计时计费系统","±1s","0 ～ 5000s","门",25,"1年","交换机分机门数：\n200门（含200门）以下 "]
[null,null,"±1s","0 ～ 5000s","门",15,"1年","交换机分机门数：200门以上  "]
["SP-010-209","单机型和集中管理分散计费型电话计时计费器","±1s","0 ～ 5000s","台",100,"1年","单机型  "]
[null,null,"±1s","0 ～ 5000s","路",80,"1年","集中管理分散计费型 "]
["WH-001-210","酸度计","0.02 ～ 0.001级                           ","pH：0 ～ 14","台",200,"1年"]
["WH-002-211","酸度计检定仪","0.0006级","0 ～ 2V","台",525,"1年"]
["WH-003-212","原子吸收分光光度计","Cu：1.5% ～ 5%\nCd：4% ～ 10%","0.00 ～ 5.00μg/mL\n0.00 ～ 5.00ng/mL","台",700,"2年"]
["WH-004-213","冷原子吸收测汞仪","±15%","（1 ～ 10）μg/L","台",470,"1年"]
["WH-005-214","单光束紫外可见分光光度计","0.5 ～ 2.0nm，A、B级","波长：190 ～ 850nm ","台",500,"1年"]
["WH-006-215","双光束紫外可见分光光度计","0.5 ～ 1.0nm，A、B级","波长：190 ～ 900nm ","台",770,"1年"]
["WH-007-216","紫外可见近红外分光光度计","0.3 ～ 2.0nm，A、B、C级","波长：185 ～ 2600nm ","台",500,"1年"]
["WH-008-217","可见分光光度计","1 ～ 3nm，一、二、三级","波长：330 ～ 800nm ","台",500,"1年"]
["WH-009-218","火焰光度计",0.032,"K：0.004 ～ 0.20mmol/L\nNa：0.004 ～ 1.00mmol/L","台",280,"1年"]
["WH-010-219","硝酸根自动监测仪",0.1,"1 ～ 100mg/L","台",440,"1年"]
["WH-011-220","水质综合分析仪","pH：0.01",null,"台",1155,"1年","测酸度、电导、浊度三参数"]
["WH-012-221","生物化学需氧量测定仪",0.05,"0 ～ 700mg/L","台",630,"1年"]
[null,"生物化学需氧量（BOD5）测定仪",0.05,"0 ～ 700mg/L","台",595,"1年"]
["WH-013-222","溶解氧测定仪","0.5mg/L","0 ～ 20mg/L","台",1120,"1年"]
["WH-014-223","干涉滤光片","0.2nm，一级","可见光区","片",240,"1年"]
["WH-015-224","可见光透射比滤光片","±1%","0 ～ 100%","片",225,"1年"]
["WH-016-225","紫外光透射比滤光片","±1%","0 ～ 100%","片",240,"1年"]
["WH-017-226","CO，CO2红外线气体分析仪","1% ～ 5%","0～100% （两种气体）","种",525,"1年"]
["WH-018-227","可燃气体测报仪（甲烷）","5%，10%","0～100% LEL","台",450,"1年"]
["WH-019-228","硫化氢气体测报仪","3% ～ 5%","0 ～ 500×10-6","台",665,"1年"]
["WH-020-229","二氧化硫分析仪","3% ～ 5%","0 ～ 4000×10-6","台",400,"1年"]
["WH-021-230","汽车排放气体测试仪","3% ～ 5%","CO：0 ～ 10%\nCH：0 ～ 1% mol/mol","台",1250,"1年"]
[null,null,"±10%","CO：0 ～ 10%\nCH：0 ～ 1% mol/mol","台",750,"1年"]
["WH-022-231","烟尘测量仪","2.5级","≤ 60L/min","台",510,"1年"]
["WH-023-232","测氢仪","±3%","0 ～ 10×10-6（质量分数）","台",280,"1年"]
["WH-024-233","血细胞分析仪","5% ～ 10%","RBC：（2.5 ～ 6.5）×1012个/L\nWBC：（2 ～ 14）×109个/L\nHD：50 ～ 200g/L","台",470,"1年"]
["WH-025-234","呼出气体酒精含量探测器",null,null,"台",300,"1年"]
["WH-026-235","通风干湿表","2%RH","（10 ～ 98）%RH","台",700,"1年"]
["WH-027-236","二级标准粘度液","二级","（1 ～ 105）mm2/s","温度点",1000,"2年","动力粘度  "]
["WH-028-237","毛细管粘度计（标准器）","0.15% ～ 0.6%，标准","1 ～ 105mm2/s","支",1410,"2年"]
[null,"毛细管粘度计（工作）","0.3% ～ 1%，工作","0.40 ～ 6.0mm","支",200,"2年"]
["WH-029-238","糖量计","一等","0 ～ 80%","点",30,"1年"]
[null,null,"工作","0 ～ 80%","点",20,"1年"]
["WH-030-239","乳汁计","工作用","15 ～ 40度","点",20,"1年"]
["WH-031-240","露点仪","±3℃DP","（-80 ～ 20）℃DP","台",1500,"1年"]
["WH-032-241","低温露点仪","±2℃DP","（-80 ～ 0）℃DP","台",1500,"1年"]
["WH-033-242","碳露点仪","±2℃DP","（-30 ～ 30）℃DP","台",1500,"1年"]
["WH-034-243","标准露点仪","一级","（-70 ～ 20）℃","台",1750,"1年"]
["WH-035-244","二级标准湿度发生器","±2%RH","（10 ～ 95）%RH","台",2800,"1年"]